Aluminium Frame Neo Advance® Flat Opening Rooflight units \_\_ degree flat roofs

1. Manufacturer: The Rooflight Co.
   1. Contact Details
      1. Address: Unit T1 Bourton Industrial Park

Bourton-on-the-Water

Cheltenham

GL54 2HQ

* + 1. Telephone: +44 (0) 1993 833155
    2. Web: [www.therooflightco.com](http://www.therooflightco.com)
    3. Email: [hello@therooflightco.com](mailto:hello@therooflightco.com)
  1. Product Reference: Neo Advance Flat Opening (NFO\_\_\_)

1. Product Performance
   1. Whole Window U-Value: 1.43W/m2K
2. Frame
   1. Material: Patented Aluminium Frame (as per GB2586514 and GB2586515)
   2. Finish
      1. Corrosion Protection: EN 60068-2-11 to classification 1440hrs (60 days).
      2. Coating: Polyester Powder Coating
      3. Colour: RAL 7022 Smooth Semi-Gloss Umbra Grey
3. Kerb Installation: As per manufacturer’s recommendations
4. Glazing or Infill
   1. Standards/Type: BSI Kitemarked (KM93754) Insulated glazing units to EN1279
   2. Construction: 6HT (16 Argon 90) 33.1
   3. Colour: Clear
   4. Acoustic Performance of Glazing: 36 (-2; -5) dB to EN12758
5. Operation
   1. Operation Type: Motorised opening with concealed motors at rooflight cill to stroke length 300mm.
6. Accessories: N/A
7. Glazing Bars: N/A
8. Third Party Certification: N/A