Aluminium Frame Neo Advance® Flat Opening Rooflight units \_\_ degree flat roofs

1. Manufacturer: The Rooflight Co.
	1. Contact Details
		1. Address: Unit T1 Bourton Industrial Park

 Bourton-on-the-Water

 Cheltenham

 GL54 2HQ

* + 1. Telephone: +44 (0) 1993 833155
		2. Web: [www.therooflightco.com](http://www.therooflightco.com)
		3. Email: hello@therooflightco.com
	1. Product Reference: Neo Advance Flat Opening (NFO\_\_\_)
1. Product Performance
	1. Whole Window U-Value: 1.43W/m2K
2. Frame
	1. Material: Patented Aluminium Frame (as per GB2586514 and GB2586515)
	2. Finish
		1. Corrosion Protection: EN 60068-2-11 to classification 1440hrs (60 days).
		2. Coating: Polyester Powder Coating
		3. Colour: RAL 7022 Smooth Semi-Gloss Umbra Grey
3. Kerb Installation: As per manufacturer’s recommendations
4. Glazing or Infill
	1. Standards/Type: BSI Kitemarked (KM93754) Insulated glazing units to EN1279
	2. Construction: 6HT (16 Argon 90) 33.1
	3. Colour: Clear
	4. Acoustic Performance of Glazing: 36 (-2; -5) dB to EN12758
5. Operation
	1. Operation Type: Motorised opening with concealed motors at rooflight cill to stroke length 300mm.
6. Accessories: N/A
7. Glazing Bars: N/A
8. Third Party Certification: N/A