Steel frame Conservation Plateau Rooflight units \_\_\_\_ degree pitched roofs

1. Manufacturer: The Rooflight Co.
   1. Contact Details
      1. Address: Unit T1 Bourton Industrial Park

Bourton-on-the-Water

Cheltenham

GL54 2HQ

* + 1. Telephone: +44 (0) 1993 833155
    2. Web: [www.therooflightco.com](http://www.therooflightco.com)
    3. Email: [hello@therooflightco.com](mailto:hello@therooflightco.com)
  1. Product Reference: Conservation Plateau Rooflight (PL\_\_\_)

1. Product Performance
   1. Whole Window U-Value: 1.8W/m2K
2. Frame
   1. Material: Steel Frame
   2. Finish
      1. Corrosion Protection: EN ISO 12944 to classification C5-M Long.
      2. Coating: Polyester Powder Coating
      3. Colour: RAL 9005 Semi Textured Black
3. Kerb Installation: As per manufacturer’s recommendations
4. Glazing or Infill
   1. Standards/Type: BSI Kitemarked (KM93754) Insulated glazing units to EN1279-3
   2. Construction: 4HT (16 Argon 90) 33.1
   3. Colour: Clear
   4. Acoustic Performance of Glazing: 34 (-1; -5) dB to EN12758
5. Operation
6. Operation Type: Brass Winder/Chrome Winder/ Brass Winder and wheel/ Chrome winder and wheel/Brass Winder with out of reach handle / Chrome Winder with out of reach handle/Motorised opening to stroke length mm [Delete as Appropriate]
7. Accessories: Extension pole and winding crank/ N/A [only applicable for manual out of reach opening option. Delete as appropriate]
8. Glazing Bars: To manufacturer’s specification.
9. Third Party Certification: BSI Kitemark on glazing KM93754.