Steel frame Neo Rooflight units \_\_\_\_ degree pitched roofs

1. Manufacturer: The Rooflight Co.
	1. Contact Details
		1. Address: Unit T1 Bourton Industrial Park

 Bourton-on-the-Water

 Cheltenham

 GL54 2HQ

* + 1. Telephone: +44 (0) 1993 833155
		2. Web: [www.therooflightco.com](http://www.therooflightco.com)
		3. Email: hello@therooflightco.com
	1. Product Reference: Neo Rooflight (Neo \_\_\_)
1. Product Performance
	1. Whole Window U-Value: 1.4W/m2K
2. Frame
	1. Material: Patented Steel Frame (as per GB251419)
	2. Finish
		1. Corrosion Protection: EN ISO 12944 to classification C5-M Long.
		2. Coating: Polyester Powder Coating
		3. Colour: RAL 7022 Smooth Semi-Gloss Umbra Grey
3. Glazing or Infill
	1. Standards/Type: BSI Kitemarked (KM93754) Insulated glazing units to EN1279-3
	2. Construction: 4HT (16 Argon 90) 4HT
	3. Colour: Clear
	4. Acoustic Performance of Glazing: 31 (-1; -4) dB to EN12758
4. Operation
	1. Operation Type: Fixed Closed/ Brushed Stainless Steel Manual Handle/ Motorised Opening with Concealed Jamb Motors to stroke length of 150/300/450mm/ Motorised Opening with Concealed Cill Motor to stroke length of 150/300/450mm [Delete as Appropriate]
5. Accessories: Concealed Gas Struts/ N/A [Delete as appropriate. Select N/A if fixed closed opening option is selected.]
6. Glazing Bars: N/A
7. Third Party Certification: Conformity Marking in accordance with EN 14351-1. BSI Kitemark on glazing KM93754.